**PROFESSIONAL COATINGS**

**PRODUCT DESCRIPTION:**

VSC SEAM TAPE is ideally suited for use with ?PRODUCTS?. They quickly wetout and saturate the fiber structure of the fleece backing. These properties ensure a true monolithic membrane which remains intact even under thermal shock conditions.

VSC SEAM TAPE provides good elongation and maintains its elasticity at extremely low temperatures. It cannot be stretched in the uncoiling direction, but can be easily stretched or formed across the web. It has no elastic memory and will not creep, allowing it to remain exactly where it is placed.

**RECOMMENDED USAGE**:

Reinforcement of seams, cracks and penetrations on various roofing surfaces:

\* Galvanized and painted Metal

\* Single ply roofing

\* Concrete

\* Modified Bitumen

**PACKAGING INFORMATION:**

2” x 50’ tape roll

**APPLICATION:**

Simply line up the two adjoining areas to be sealed, with the release paper still attached, then start removing the release paper from the underside and placing the membrane close to the desired position. It can then be worked into all cracks and crevices using your fingers, a blunt awl, or plastic knife.

**CLEAN UP:**

Use SOLVENT 101 or Xylol to clean tools immediately after installation. Follow product guidelines for safe use. Must allow adequate ventilation.

**DISPOSAL:**

Empty containers may contain product residue, including flammable or combustible vapors. Do not cut, puncture or weld near these containers. Label warnings must be observed until containers have been commercially cleaned or reconditioned. Containers to be thrown out must be disposed of in accordance with federal, state and local regulations. Use only licensed hazardous waste disposal companies if required.

**PRECAUTIONS:**

Carefully read product labels, application guidelines and Material Safety Data Sheet before using all products. Contact with liquids may cause irritation. Use appropriate safety gear including eye protection. Must allow adequate ventilation.

**ADDITIONAL INFORMATION:**

For additional information or application help regarding this product or others please contact Vanberg Specialized Coatings at **1-800-874-0631** or **www.vanbergcoatings.com**

.

|  |  |
| --- | --- |
| **GENERAL PRODUCT DATA** | |
| **FEATURE** | **ADVANTAGE** |
| **SOLIDS CONTENT** | 99.8% (ASTM D-1729-69) |
| **MOISTURE VAPOR TRANSMISSION** | .75 perms |
| **Elongation webbing** | 200% min. |
| **Tensile Strength** | 35 PSI (ASTM D-412) |
| **Cold temp FLEXIBILITY** | Passes |