**PROFESSIONAL COATINGS**

**PRODUCT DESCRIPTION:**

This solvent-based acrylic quickly penetrates and provides a thorough, durable seal or finish coating. Very good gloss retention. Resists oils, water vapor, alkali and acids. Seals concrete preventing dusting. Prevents pitting and staining. Does not discolor when exposed to UV light. Because it dries quickly, down time is kept to a minimum.

**RECOMMENDED USES:**

Use on concrete, masonry, stone wash, stone and terrazzo. Excellent for factories, livestock facilities, warehouses, garages, maintenance areas, parking lots, sidewalks, driveways, etc. High traffic areas can be easily recoated and maintained. Should not be used on linoleum, asphalt tile, vinyl asbestos tile, rubber or quarry tile.

**COVERAGE:**

Approximately 400 sq. ft. per gallon.

**PACKAGING:**

* 55-gallon unit (445 lbs)
* 5-gallon unit (37 lbs) #CS510-5
* 1-gallon jugs 4/cs (7.4 lbs.) #CS510-1

**APPLICATION:**

Roller or Spray (Use a metal pump up solvent resistant sprayer with Viton gaskets). Clean up with SOLVENT 101 or Xylol.

**DOT DESCRIPTION:**

PAINT (FLAMMABLE LIQUID)

3, UN 1263, II

**HMIS:**

Health - 2

Flammability – 3

Reactivity – 0

**NFPA:**

Health –

Reactivity – 0

Flammability – 3

|  |  |
| --- | --- |
| PHYSICAL PROPERTIES | |
| FORM | LIQUID |
| **ODOR** | AROMATIC SOLVENT |
| **COLOR** | COLORLESS |
| **CLARITY** | CLEAR |
| **SEDIMENT** | NONE |
| **STABILITY** | 1 YEAR MINIMUM |
| **COLD STABILITY** | NOT AFFECTED |
| **BOILING POINT** | 230°F |
| **pH** | N/A |
| **SPECIFIC GRAVITY** | .89 |
| **POUNDS/GALLONS** | 7.4 |
| **SOLIDS** | 15.0 |
| **FLASH POINT** | 45°F |
| **COVERAGE** | 300-400 sq. ft./gal. |